Model:F7

ZKTeco Biometric RFID Fingerprint Time Attendance clock IP/TCP Access Control

Model:F18

ZKTeco fingerprint reader fingerprint access control to exit and enter the full access control door system with software

Model:F22

ZKTeco Ultra thin Fingerprint Time Attendance & Access Control System

Model:F302

ZKTeco Face Detection and Time Attendance Access Control

Model:20C

One Single Door RFID Card Access Control Keypad

Model:T12

One Single Door RFID Card Access Control Keypad

Model:Breakglass

Emergency Break Glass For Door Access

Model:Door Exit

PC Fireproof Plastic Door Exit Push Release Button Switch for Electric Access Control (White)

Model:EM Lock

High-Quality Industrial Grade Metal Electro Magnetic Lock/EM Lock Single Leaf 12V DC

Model:LZ Bracket

EM Lock LZ Bracket For Door Access Use

Model: RFID-C

White Plastic Contactless 125kHz TK4100 EM4100 RFID Proximity ID Smart Entry Access Card

Model:U Bracket

U-Bracket for Door Access Use

Model:Battery 12v/7A

12V7AH Battery 12V access control battery 12V alarm spare battery UPS battery

Modedl:PS5A12V-Door Access

DC13.5V 5A Uninterrupted Power Supply using Access Control System UPS Power Supply AC 220V

Model:RFID-KC

Access Card Key Chain RFID Keyfob Proximity 125KHZ TK / EM4100 Tag ID

Model:FS601

Waterproof Metal Keypad RFID Access Control System Proximity Card Standalone 2000 Users Door Access Control

Model:DS-K1T804MF

HIKVISION, LCD Display, STANDALONE TIME/ATTENDANCE/Access Terminal, MIFARE and Fingerprint Reader